**INSTALLATION INSTRUCTIONS**

JEEP JK STABILIZER KIT

1. **Remove the factory stabilizer from the axle**
2. **Remove the factory track bar from the axle mount**
3. **Place the new bracket on the axle mount and place the track rod in the axle mount and secure with the factory track rod bolt. Do not tighten at this time.**
4. **Install on the stabilizer bracket and tighten hardware.**
5. **Install stabilizer in the mount**
6. **loosen the tie rod mount and rotate it so the stabilizer mounting bolt is pointing upward. Snug the tie rod mount.**
7. **Attach the stabilizer to the mount**
8. **Turn the wheels all the way to the right and adjust the tie rod mounting bracket so that there is only 1” of the stabilizer shaft showing. Tighten the tie rod mounting bracket**
9. **Perform a steering sweep, by moving the steering from lock to lock, to make sure the stabilizer does not come in contact with anything.**





